<?xml version="1.0" encoding="UTF-8"?>
<!--Internal Information used to aid in debugging customer issues:
Build Version: 4.0000
License Information: Flexlm License: (GTise/31-oct-2015)  GT-SUITE workstation: (PC-723-11)  License Server: (ls12120.fsid.cvut.cz) vend: (UJERHESCAMJFTEALMKVCITUQLCQYAB)
Important Files		Last Modified Date (Build Number)
GTsuite_dp.exe		12/4/2014 2:24:36 odp. (4.0000)
GTsuite_RT_dp.exe		12/3/2014 8:29:28 dop. (4.0000)
GTsuite_mp.exe		12/4/2014 2:24:48 odp. (4.0000)
gtise.jar		12/2/2014 4:17:40 odp. (4.0000)
gtpost.jar		12/10/2014 11:18:42 dop. (4.0000)
vtdesign.jar		12/2/2014 4:13:21 odp. (4.0000)
gem.jar		12/2/2014 4:09:32 odp. (4.0000)
gtise740.gtt		12/4/2014 1:31:32 odp. (4.0000)
resources.jar		12/2/2014 4:12:35 odp. (4.0000)
gtdatacollector.jar		12/10/2014 11:18:42 dop. (4.0000)
solverjni.jar		12/2/2014 4:46:05 odp. (4.0000)
gtsuitejni.dll		12/4/2014 3:50:52 odp. (4.0000)
gtise_help.jar		12/1/2014 9:22:30 odp.
japanese_gtise_help.jar		11/20/2014 7:49:56 dop.
gtpost_help.jar		12/1/2014 10:32:16 odp.
cool3d_help.jar		12/1/2014 10:49:40 odp.
gem3d_help.jar		12/1/2014 11:11:18 odp.
vtdesign_help.jar		12/1/2014 10:40:28 odp.
gtexecconfigeditor_help.jar		12/1/2014 10:51:48 odp.
gtscheconfigeditor_help.jar		12/1/2014 10:53:44 odp.

System Properties:
GTIHOME Environment Variable: C:\GTI
GTISOFT LICENSE FILE: 27005@ls12120.fsid.cvut.cz
LCTYPE: null
PATH Environment Variable: C:\GTI\v7.4.0\GTsuite\bin\win32;C:\GTI\bin;C:\Program Files\PC Connectivity Solution;C:\GTI\bin;C:\Program Files\NVIDIA Corporation\PhysX\Common;C:\GTI\bin;C:\GTI\bin;C:\WINDOWS\system32;C:\WINDOWS;C:\WINDOWS\system32\wbem;C:\Program Files\Pinnacle\Shared Files;C:\Program Files\MATLAB\R2010b\runtime\win32;C:\Program Files\MATLAB\R2010b\bin;C:\WINDOWS\system32\WindowsPowerShell\v1.0;C:\Program Files\Platform Computing\Platform-MPI\bin;C:\Program Files\QuickTime Alternative\QTSystem;C:\Program Files\CONVERGE;C:\Program Files\Calibre2;C:\GTI\bin\win32;
Java Runtime Environment version: 1.7.0_09
Java Runtime Environment vendor: Oracle Corporation
Java installation directory: C:\GTI\v7.4.0\GTsuite\jre\win32
Java Virtual Machine specification version: 1.7
Java Virtual Machine implementation version: 23.5-b02
Java maximum heap: 1524m
Operating system name: Windows XP
Operating system architecture: x86
Operating system version: 5.1
Native compiler switch: win32
Native library build: 4.0000
System library path: N/A
Database mode: Global mode
Database port: 50050
Database directory: d:\temp\gtidata\dbdir
Direct Draw: false
Direct Draw OffScreen: false
Skip Java Paint Manager: true
Video Adapter: Not checked on Linux systems.
Java3D version : java3d is not supported here anymore!
JMF    version : 2.1.1e
Video driver not found or needs update-->
<file code="GT-SUITE 7.4.0" develop_ver="740002" dfltfile="$GTIHOME$\v7.4.0\resrc\gtpower.gpd" maingb="iveco_1_37s_T1-indi12-V74_optim_boost.gdx" name="iveco_1_37s_T1-indi12-V74_optim_boost" type="gu" version="7.4.0">
    <case DEV_DISABLE_CLONE="1" caseno="1" name="New Case" state="0" type="std">
        <group layout="2x2" name="Srovnani - vykony" state="0" type="group">
            <plot flegdpos="top" label1="" name="Brake Power (kW)" plottype="xy" rlt="on" rlt_symbol="bkw" sn="" state="0" t_id="154" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Power [UNIT]" yunit="104">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#bkw:Engine" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#bkw:Engine" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="Power" state="0" type="excel" xunit="139" yunit="104">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="13" rowstart="13" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="Brake Torque" plottype="xy" rlt="on" rlt_symbol="btq" sn="" state="0" t_id="154" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Torque [UNIT]" yunit="115">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#btq:Engine" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#btq:Engine" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="TORQUE" state="0" type="excel" xunit="139" yunit="115">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="14" rowstart="14" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="BMEP - Brake Mean Effective Pressure" plottype="xy" rlt="on" rlt_symbol="bmep" sn="" state="0" t_id="154" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="BMEP [UNIT]" yunit="25">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#bmep:Engine" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#bmep:Engine" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="BMEP" state="0" type="excel" xunit="139" yunit="25">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="15" rowstart="15" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="IMEP720 - Net Indicated Mean Effective Pressure" plottype="xy" rlt="on" rlt_symbol="imep" sn="" state="0" t_id="154" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Net IMEP [UNIT]" yunit="25">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#imep:Engine" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#imep:Engine" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
            </plot>
            <plot disable_multiple_legend_y="false" flegdpos="top" label1="" name="Mechanical Efficiency" plottype="xy" rlt="on" rlt_symbol="bmep" sn="" state="0" t_id="154" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xdectype="auto" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" y2_axis_order="47" y2_location="east" y2label="EFF_MECH [UNIT]" y2lineslcol="25" y2lineslthk="1" y2linesltyp="dashed-1" y2rangmaxtype="user" y2rangmaxuser="100.0" y2rangmintype="user" y2rangminuser="60.0" ydectype="auto" ylabel="Mechanical Efficiency (Unit conflict )" ylineslcol="25" ylineslthk="1" ylinesltyp="dashed-1" yrangmaxtype="user" yrangmaxuser="100.0" yrangmintype="user" yrangminuser="60.0" yunit="0">
                <data datatype="xy" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" mathoper="user" name="iveco_Rcube2-indi14" state="0" type="math" user_eq="BMEP/IMEP*100" xunit="139" yunit="0">
                    <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#bmep:Engine" mathchild="on" name="iveco_1_37s_T1-indi12-V74_optim_boost" state="1" type="imp"/>
                    <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#imep:Engine" mathchild="on" name="iveco_1_37s_T1-indi12-V74_optim_boost" state="1" type="imp"/>
                </data>
                <data caseno="0" datatype="xy" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" mathoper="user" name="iveco_rCube2-indi14-FRM_step11" state="0" type="math" user_eq="BMEP/IMEP*100" xunit="139" yunit="0">
                    <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#bmep:Engine" mathchild="on" name="iveco_1_37s_T1-indi12-V74_optim_boost" state="1" type="imp"/>
                    <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#imep:Engine" mathchild="on" name="iveco_1_37s_T1-indi12-V74_optim_boost" state="1" type="imp"/>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="BSFC - Brake Specific Fuel Consumption, Cyl" plottype="xy" rlt="on" rlt_symbol="bsfc" sn="" state="0" t_id="154" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="BSFC [UNIT]" ylineslcol="25" ylineslthk="1" ylinesltyp="dashed-1" yrangmaxtype="user" yrangmaxuser="240.0" yrangmintype="user" yrangminuser="190.0" yunit="125">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#bsfc:Engine" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#bsfc:Engine" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="BSFC" state="0" type="excel" xunit="139" yunit="125">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="23" rowstart="23" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="Maximum Cylinder Pressure" plottype="xy" rlt="on" rlt_symbol="cylpmav" sn="" state="0" t_id="154" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Pressure [UNIT]" yunit="25">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#cylpmav:Engine" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#cylpmav:Engine" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="PMAX1" state="0" type="excel" xunit="139" yunit="25">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="25" rowstart="25" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot label1="" name="Injected Mass per Cycle" plottype="xy" rlt="on" rlt_symbol="injrat" sn="" state="0" t_id="56" use_default_unit_x="false" use_default_unit_y="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Mass per Cycle [UNIT]" yunit="252">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" flinethk="2" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#injrat:di-inject-01" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#injrat:di-inject-01" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" fsymbol="triangle" fsymbsize="9" name="Fuel Injected (from fuel flow rate)" state="0" type="excel" xunit="139" yunit="252">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="27" rowstart="27" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
        </group>
        <group layout="2x2" name="Srovnani tlaky teploty" state="0" type="group">
            <plot flegdpos="top" label1="" name="Air Pressure" plottype="xy" rlt="on" rlt_symbol="pav" sn="" state="0" t_id="4" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Pressure [UNIT]" yunit="25">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pav:env" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pav:env" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="P_AIR" state="0" type="excel" xunit="139" yunit="25">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="49" rowstart="49" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="Air Temperature" plottype="xy" rlt="on" rlt_symbol="tav" sn="" state="0" t_id="4" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Temperature [UNIT]" ylineslcol="25" ylineslthk="1" ylinesltyp="dashed-1" yunit="34">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#tav:env" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#tav:env" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="T_AIR" state="0" type="excel" xunit="139" yunit="34">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="50" rowstart="50" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="p2C" plottype="xy" rlt="on" rlt_symbol="pavr" sn="" state="0" t_id="19" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Pressure [UNIT]" yunit="25">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pavr:in_sys_bend_03" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pavr:in_sys_bend_03" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="P_IC_IN" state="0" type="excel" xunit="139" yunit="25">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="100" rowstart="100" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="t2C" plottype="xy" rlt="on" rlt_symbol="tavr" sn="" state="0" t_id="19" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Temperature [UNIT]" yunit="34">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#tavr:in_sys_bend_03" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#tavr:in_sys_bend_03" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="T_IA_TC" state="0" type="excel" xunit="139" yunit="34">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="101" rowstart="101" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="top" label1="" name="p1E" plottype="xy" rlt="on" rlt_symbol="pavl" sn="" state="0" t_id="21" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Pressure [UNIT]" yunit="25">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pavl:in_sys_bend_07" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pavl:in_sys_bend_07" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="P_IC_OUT" state="0" type="excel" xunit="139" yunit="25">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="59" rowstart="59" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="t1E" plottype="xy" rlt="on" rlt_symbol="tavr" sn="" state="0" t_id="21" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Temperature [UNIT]" yunit="34">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#tavr:in_sys_bend_07" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#tavr:in_sys_bend_07" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="T_IM" state="0" type="excel" xunit="139" yunit="34">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="60" rowstart="60" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="p1T" plottype="xy" rlt="on" rlt_symbol="pav" sn="" state="0" t_id="17" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Pressure [UNIT]" yunit="25">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pav:exh_man_fs_leakag-01" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pav:exh_man_fs_leakag-01" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="P_EXH" state="0" type="excel" xunit="139" yunit="25">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="108" rowstart="108" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="t1T" plottype="xy" rlt="on" rlt_symbol="tav" sn="" state="0" t_id="17" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Temperature [UNIT]" yunit="34">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#tav:exh_man_fs_leakag-01" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#tav:exh_man_fs_leakag-01" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="T_EXH" state="0" type="excel" xunit="139" yunit="34">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="109" rowstart="109" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="top" label1="" name="p2T" plottype="xy" rlt="on" rlt_symbol="pavr" sn="" state="0" t_id="19" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Pressure [UNIT]" yunit="25">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pavr:exh_sys_bend_01" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pavr:exh_sys_bend_01" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="P_33" state="0" type="excel" xunit="139" yunit="25">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="110" rowstart="110" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="t2T" plottype="xy" rlt="on" rlt_symbol="tavr" sn="" state="0" t_id="19" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Temperature [UNIT]" yunit="34">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#tavr:exh_sys_bend_01" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#tavr:exh_sys_bend_01" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="T_EXH_TC" state="0" type="excel" xunit="139" yunit="34">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="111" rowstart="111" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
            <plot flegdpos="off" label1="" name="p1T potrubi" plottype="xy" rlt="on" rlt_symbol="pav" sn="" state="0" t_id="17" use_default_unit_cn="false" use_default_unit_x="false" use_default_unit_y="false" use_default_unit_y2="false" use_default_unit_z="false" x_axis="avgrpm:Engine" xlabel="Engine Speed [UNIT]" xnowrap="on" xunit="139" ylabel="Average Pressure (Outlet) [UNIT]" yunit="25">
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="2" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pav:exh_man_fs_leakag-01" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pav:exh_man_fs_leakag-01" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_Rcube2-indi14.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pavr:exh_man_pipe-03" name="iveco_Rcube2-indi14" state="0" type="imp"/>
                <data caseno="0" datatype="xy" dbname="iveco_rCube2-indi14-FRM_step11.gdx" fcolor="3" flinethk="2" frameid="-1" fsymbol="circle" fsymbsize="9" index="avgrpm:Engine#pavr:exh_man_pipe-03" name="iveco_rCube2-indi14-FRM_step11" state="0" type="imp"/>
                <data axis_association="y1_axis" datatype="xy" fcolor="4" flinethk="2" flinetype="dashed-2" frameid="-1" fsymbol="triangle" fsymbsize="9" name="P_EXH" state="0" type="excel" xunit="139" yunit="25">
                    <list>
                        <x colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="11" rowstart="11" sheet="Test Data (Fired)" type="allowgap"/>
                        <y colend="-100" colstart="4" file="..\4.1 - TPA komplet model-Rcube2\20140206_00_WAVE_Input_Data_Iveco_indiCOM_uprav.xls" rowdata="true" rowend="108" rowstart="108" sheet="Test Data (Fired)" type="allowgap"/>
                    </list>
                </data>
            </plot>
        </group>
        <cluster name="New Report Group1"/>
    </case>
</file>
