| CASE #  1
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      9.72331727E-02   69.188898      0.82633145       39.658387    

| CASE #  2
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      6.33302380E-02   45.005922      0.79668381       29.885743    

| CASE #  3
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      3.07638383E-02   21.455220      0.74694794       19.980744    

| CASE #  4
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      4.78466968E-04 -0.97944622      0.70400328       9.9999018    

| CASE #  5
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      1.35531812E-02  -11.009162      0.77159229       6.0017538    

| CASE #  6
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      0.16256034       115.98029      0.82324859       39.290038    

| CASE #  7
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      0.10652038       75.880743      0.79415377       29.752424    

| CASE #  8
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      5.04760820E-02   35.285241      0.74503415       19.957434    

| CASE #  9
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      3.29736786E-03  -4.6953706      0.75016143       10.000012    

| CASE # 10
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      2.57376648E-02  -20.795663      0.77650459       6.0049831    

| CASE # 11
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      0.24947611       177.06647      0.81708474       38.674283    

| CASE # 12
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      0.15765882       112.14853      0.79225416       29.552804    

| CASE # 13
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      6.81165025E-02   47.693454      0.74262586       19.932333    

| CASE # 14
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      1.46094711E-02  -13.357692      0.78017298       10.001179    

| CASE # 15
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      4.57454904E-02  -35.354303      0.78151989       6.0098054    

| CASE # 16
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      0.27693966       199.19314      0.81145848       38.597574    

| CASE # 17
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      0.18151687       130.58462      0.79114208       29.510804    

| CASE # 18
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      8.36459367E-02   58.676973      0.74106260       19.911539    

| CASE # 19
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      2.71227295E-03  -7.9296627      0.73171961       9.9980569    

| CASE # 20
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      5.52024789E-02  -45.854513      0.79262735       6.0146194    

| CASE # 21
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      0.38141062       272.21729      0.79316301       37.495345    

| CASE # 22
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      0.25453214       182.00161      0.78035621       29.108032    

| CASE # 23
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      0.11338186       79.020603      0.73920651       19.867178    

| CASE # 24
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      6.46841108E-02  -53.720517      0.80042329       10.010075    

| CASE # 25
| Cyc.Angle      steam_MFR       expander_power  isentropic_effi pressure_ratio 
| deg            kg/s            kW              No Unit         No Unit        
  340.00000      0.13503948      -99.780504      0.79952564       6.0431764    

