|* GTSUITE [Version 2016.3.9589]
|===DATA FILE for GTSUITE [Version 2016.3]=====================================
| LOCDIR:  D:\DOKUMENTY\AICTA\2015 - parní stroj\GT-model - 1valec\optim 0.25kgps\optim_steam_expander-500RPM_025kgps_eff_DOS_00001_optimum
| PROJECT: ID544-Steam-expander_WATER_v08_komplet_walltemp_cylsoln_2_simple_v3-singlecyl.sim : GTSUITE
| DATE:    Pátek, září 30, 2016
| TIME:    10:25:55
| CREATOR: GTSUITE [Version 2016.3]
| GTise Build: 3.1001  gtt Build: 3.0000
|===RUN SPECIFICATIONS=========================================================
TimeControl_S -----------------------------------------------------------[582]
|TIMCYC DURATN MINDURATN DURATN2 MINDURATN2 FLUIDSS new2 MAINDRV MAINDRVREF NEWTSTEP 
 periodic 100 25 ign ign on on ign ign off
Initialization_S --------------------------------------------------------[582]
|ISTATE PARTATTR RTLSOUTPUT RLTFILE RLTCASE FILE_NAME_READ_INIT FILE_NAME_READ 
 user_imposed on ign ign ign ign ign
FlowControl_S -----------------------------------------------------------[582]
|%4 PARTS TIMCYCLFLW ISOLN MERGECIRC 
# 1
% def ign ExplicitControl off 
ODEControl_S ------------------------------------------------------------[582]
|%13 MECPARTS TIMCYCL MATXNORDOPT INTTYPE SOLCOBJ IDYNOUT MERGEMECCIRC FMSSD FMSSV FMSSF JMSSPERD MOAP MORP 
# 1
% def ign Cuthill-McKee Explicit-Runge-Kutta Explicit-def def on ign ign def 1 ign ign 
SignalControl_S ---------------------------------------------------------[582]
|%3 CNTPARTS STEPSIZE FIXEDSIZE 
# 0
ThermalControl_S --------------------------------------------------------[582]
|HTSS DTHT HTSSTTOL DFSKIP NHTSKIP IHEATCSKIP 
 "[HTSS]" def ign ign ign def
ConvergenceRLT_S --------------------------------------------------------[582]
|%8 TRLTVAR CONVACTIVE RLTFLAG1 RLTTARG RLTMULT RLTTOLTYP USRTOL NCYCRLT 
# 1
% airflow:CrankTrain-1 on RLT_interval ign def fractional 0.007 10 
General_A ---------------------------------------------------------------[582]
|EXTPARAM IMPORTEXT TSFXTRT SEED CONVEXCLLIST 
 ign "GT-ISE (only overwrite *)" ign def ign
Flow_A ------------------------------------------------------------------[582]
|BENDTABLE EQUICAL NMW AFSTREF OUTPUT2NDLAW DEADSTATE PIPECFL FSPLCFL STABLECYL CYLFLOW LIMIT_CYL_DT LIMIT_CYL_FLOW ICYLEFFANALN ITPTM ISALTLAMVLV_NEW ISALTFPDS ISNEWDIFF IMPL_RES_DEF IREFRLKP CORRECTSCPROF PTBLCMP MNMXTEMPLIMITS FMASSRT TRPFUEL MF_UNDER 
 ign off on def off ign off off on ign on off Off on off off on on on on off off off off ign
Mechanics_A -------------------------------------------------------------[582]
|GRAVITY COMPSURF 
 ign Old
Restart_A ---------------------------------------------------------------[582]
|WRITESTART WRITEINTERVAL NUM_OF_RESTART_FILES STORE_END_CASE_DATA STORE_END_SIM_DATA KEEP_RESTART_FILES 
 ign ign ign ign ign ign
VersionChanges_A --------------------------------------------------------[582]
|VERSION FLAGS NEWVALVR THICKORF2 HGLAM INJNEW2 ICDCONTRVC INITCNTCOMP ICLAMMLT IFSRIGHT VALVEPROFUPDATE PUMPVDP ILFTR ISFPDLC IJTFS CYLMAXSTEP CORRECTEDVALVETIMINGRLTS_COMBO TIMEVARIABLE SEPARATEINLAY PAVALVEHT FRAREA FLAME MTXHAAREA EVOCYLHTR LANONDEFORFTOBC PDROPREFR RESULTS2 CYLVOLOFFSET ELEINIT VALV_ARR_PRT CYLRAD VALV_TYPE_DETECT ECGBLKP FIX_TOUT_TURB ONUM_IMPL VALVDIAPRTOVRD HXMAP_LINEQ PD_CONDENSE AVGENGSPD ENDTPA FLWTHMCPL FIXFRICTURBWG XYZPULBND TRANPUDDLEFRAC THERMOPROPS EXCELUNIT RGAS_GTI FIXIMPRFRICBEND FIX_ECYL_HT_ISS FIXKNINDTIMERLT FIX_TURBRLT_2xIN EQCOMP CONV_CONT_DEA MOVINGAVG FIXHTSENSRT FIXRLTSSLAVERT ICSEOCODECIRC VOL_MPAS_HX PMEP_INTER NUMAP_ENTH INJMASSDI TRUNC_XYTABLE PRFALKPLOADMODE PROFPERIOD ACTUCOMB ENGRLTINTEG ENGSENSINTEG MPFIX CORRCYLEM LARGESTEPNOHT PIDINIT_T_U PIPWALCIRCUM CNTINDX SGPHMAINDRV INJMASSDI2 CORRECTGLCA CORRECTEULR FIXMAXAREANOTCH ENGSENSINTEG2 
 V2016 ign v72_b2 v72 on v72 on on on on on on on on on on v2016 on on on on on on on on on on on on on off on on on on on on off on on on on on on on on on on on on on off on on on on on on off ign on on off off off on on v2016b1 off off on on off off off off off off off
Paths_A -----------------------------------------------------------------[582]
|DIR 
DIR:1> ign <
MiscFiles_A -------------------------------------------------------------[582]
|%2 MISCFILES ASCBIN 
# 1
% ign ASCII 
Main_O ------------------------------------------------------------------[582]
|OPTOFF OPTADV CASEWT MAXITER TIMEOUT SAVEITERFILE OPTOLD IOPTSTAT IOPTPLOT MONITOR OPTAIM OPTMETHOD OPTVAR OPTVAL THRESVAL MAXOPT POPSIZE NUMGEN NSGAADV XORATE XODI MURATE MUDI GASEED 
 on ign ign ign ign ign ign ign ign ign ign ign ign ign ign ign ign ign ign ign ign ign ign ign
Ind_Variables_O ---------------------------------------------------------[582]
|%6 OPTIND CASEHNDL RANGE RANGEMIN RANGEMAX RESOLPERC 
# 0
Constraints_O -----------------------------------------------------------[582]
|%4 CONSTRLT LOLIMIT HILIMIT PENALTY 
# 0
Data_Storage_D ----------------------------------------------------------[582]
|DTRLTSS CaseRLTHeader1 CRLTLEVELnew CRLTLEVEL2 CRLTLIST TimeRLTHeader1 TRLTLEVELnew TRLTLEVEL2 TRLTLIST TRLTMAX RLTFREQ CRLTLIST2 PLTSUPP PLTSUP2 TBLSUPP THINNING WARNING 
 def on All All ign on All All ign 500 1 ign off off off Decimation off
General_D ---------------------------------------------------------------[582]
|NAME DTPLOT RAMRLT ENGYPLTS BRFSUPP 
 def off off off on
GT-POST_Setup_D ---------------------------------------------------------[582]
|XCASERLT XTIMERLT EXTDATAFILE EXTDATASHEET EXTFORMAT GPDFILE 
 def time ign ign ign def
Flow_D ------------------------------------------------------------------[582]
|NUMANIM MICDATA OLT NUMHARM DEWFLAG OUTPUT 
 ign ign ign def off no
ODE-Mech_D --------------------------------------------------------------[582]
|ODEPLTS MECPLTO KINPLTO EIGPLTO MECPLTO3D 
 off ign ign ign ign
ScoreboardRLTs_D --------------------------------------------------------[582]
|CrankScore CylScore TurboScore LubeScore InjScore VehScore HXScore RefrigScore 
 Engine Cylinder Turbo Lubrication Injector Vehicle HeatExchangers RefrigFlowMach
UserScoreboardRLTs_D ----------------------------------------------------[582]
|UsrScrName UsrScrRLTList 
UsrScrName:1> def <
UsrScrRLTList:1> ign <
EndOfRunTables_D --------------------------------------------------------[582]
|ISETUP PARLAB ICONFIG EORTAB_1 EORTAB_2 EORTAB_3 EORTAB_4 EORTAB_5 
 Case_Setup ign Column ign ign ign ign ign
|# 973741|973107|962668|962725|977869|973742|962785|978421|962674|
|===PLOT SPECIFICATIONS========================================================
PlotPoints --------------------------------------------------------------------
|{XLOC} PLPNT PL_RANGE XAXIS_TYPE SAMPL_TYPE SAMPL_INTERVAL INTERPOL ZEROTIME
 {0.5} 20000 Automatic Automatic Timestep 1.0 use_nearest_volume off
PlotData ----------------------------------------------------------------------
|PART# PLOT {XLOC} PLPNT PL_RANGE XAXIS_TYPE SAMPL_TYPE SAMPL_INTERVAL
66130 pres {0.5} def def def def def
66127 pres {0.5} def def def def def
66218 pres def def def def def
66215 pres def def def def def
66309 mdot {0.5} def def def def def
66309 pres {0.5} def def def def def
66291 mdot def def def def def
66291 mach def def def def def
66291 deltap def def def def def
66291 mvsl def def ign def def
66291 vel def def def def def
66291 area def def def def def
66291 masstot def def def def def
66291 lift def def def def def
66291 cd def def def def def
66285 mdot def def def def def
66285 mach def def def def def
66285 deltap def def def def def
66285 mvsl def def ign def def
66285 vel def def def def def
66285 area def def def def def
66285 masstot def def def def def
66285 lift def def def def def
66285 cd def def def def def
65894 INPT {1 2} def ign ign def def
66276 mdot def def def def def
66276 mach def def def def def
66276 deltap def def def def def
66276 mvsl def def ign def def
66276 vel def def def def def
66276 area def def def def def
66276 masstot def def def def def
66276 lift def def def def def
66276 cd def def def def def
66273 mdot {0.5} def def def def def
66273 pres {0.5} def def def def def
66264 httr def def def def def
66264 temp def def def def def
66264 hg def def def def def
66264 pres def def def def def
66264 p-v def def ign def def
66264 pmploop def def def def def
66264 httrflx def def def def def
66134 pres def def def def def
66128 pres def def def def def
66310 mdot def def def def def
66310 mach def def def def def
66310 deltap def def def def def
66310 mvsl def def ign def def
66310 vel def def def def def
66310 area def def def def def
66310 masstot def def def def def
66310 lift def def def def def
66310 cd def def def def def
66307 mdot def def def def def
66307 mach def def def def def
66307 deltap def def def def def
66307 mvsl def def ign def def
66307 vel def def def def def
66307 area def def def def def
66307 masstot def def def def def
66307 lift def def def def def
66307 cd def def def def def
66110 temp {0.5} def def def def def
66110 pres {0.5} def def def def def
66110 tsu {0.5} def def def def def
66110 qual {0.5} def def def def def
66295 mdot {0.5} def def def def def
66295 pres {0.5} def def def def def
65807 bulkms {0.5} def def def def def
65807 cs {0.5} def def def def def
65807 httr {0.5} def def def def def
65807 hgx {0.5} def def def def def
65807 mach {0.5} def def def def def
65807 vol {0.5} def def def def def
65807 twprf {0.5} def ign ign ign ign
65807 temp {0.5} def def def def def
65807 cf2 {0.5} def def def def def
65807 ucen {0.5} def def def def def
65807 twal {0.5} def def def def def
65807 hg2 {0.5} def def def def def
65807 qbal def def def def def
65807 volflow {0.5} def def def def def
65807 totp {0.5} def def def def def
65807 pres {0.5} def def def def def
65807 dynvis {0.5} def def def def def
65807 acc {0.5} def def def def def
65807 rho {0.5} def def def def def
65807 kinvis {0.5} def def def def def
65807 cp {0.5} def def def def def
65807 acc2 {0.5} def def def def def
65807 hg {0.5} def def def def def
65807 qual {0.5} def def def def def
65807 rgas {0.5} def def def def def
65807 tsu {0.5} def def def def def
65807 htactu {0.5} def def def def def
65807 temptcro {0.5} def def def def def
65807 re {0.5} def def def def def
65807 mdot {0.5} def def def def def
65807 vel {0.5} def def def def def
65807 htcro {0.5} def def def def def
65807 trav {0.5} def def def def def
65807 dt {0.5} def def def def def
65807 cond {0.5} def def def def def
65807 mint {0.5} def def def def def
65807 bulkmt {0.5} def def def def def
65807 gam {0.5} def def def def def
66283 mdot def def def def def
66283 mach def def def def def
66283 deltap def def def def def
66283 mvsl def def ign def def
66283 vel def def def def def
66283 area def def def def def
66283 masstot def def def def def
66283 lift def def def def def
66283 cd def def def def def
66277 mdot def def def def def
66277 mach def def def def def
66277 deltap def def def def def
66277 mvsl def def ign def def
66277 vel def def def def def
66277 area def def def def def
66277 masstot def def def def def
66277 lift def def def def def
66277 cd def def def def def
66271 mdot {0.5} def def def def def
66271 pres {0.5} def def def def def
66244 ts_final def def ign ign ign
66244 ts def def ign ign ign
66244 ph_final def def ign ign ign
66244 ph def def ign ign ign
66282 mdot {0.5} def def def def def
66282 pres {0.5} def def def def def
65826 temp {0.5} def def def def def
65826 pres {0.5} def def def def def
65826 tsu {0.5} def def def def def
65826 qual {0.5} def def def def def
66308 mdot {0.5} def def def def def
66308 pres {0.5} def def def def def
66102 htrates def ign ign ign ign
66102 twaltemp def ign ign ign ign
66102 pistfetemp2D def ign ign ign ign
66102 pistfetemp3D def ign ign ign ign
66102 headfetemp3D def ign ign ign ign
66102 cylfetemp3D def ign ign ign ign
66102 portfetemp3D def ign ign ign ign
66102 valvfetemp3D def ign ign ign ign
66102 httr def def def def def
66102 temp def def def def def
66102 pres def def def def def
66102 httrflx def def def def def
66102 pmploop def def def def def
66102 hg def def def def def
66102 p-v def def ign def def
66102 pistfeports def ign ign ign ign
66102 portfeports def ign ign ign ign
66102 cylfeports def ign ign ign ign
66102 headfeports def ign ign ign ign
66102 valvfeports def ign ign ign ign
66293 mdot def def def def def
66293 mach def def def def def
66293 deltap def def def def def
66293 mvsl def def ign def def
66293 vel def def def def def
66293 area def def def def def
66293 masstot def def def def def
66293 lift def def def def def
66293 cd def def def def def
66290 mdot {0.5} def def def def def
66290 pres {0.5} def def def def def
66287 mdot {0.5} def def def def def
66287 pres {0.5} def def def def def
ObjectPlotData ----------------------------------------------------------------
ValveCamConn valconexh O_PLOTFLAG_1
ValveCamConn valconexh O_PLOTFLAG_2
ValveCamConn valconexh O_PLOTFLAG_3
ValveCamConn valconint O_PLOTFLAG_1
ValveCamConn valconint O_PLOTFLAG_2
ValveCamConn valconint O_PLOTFLAG_3
FECylinderStructure tw1_detailFEM O_PLTVALV_1
XYZPoints h2s-lookup O_PLT0_1
Setup Main_O O_IOPTPLOT_1
Setup Main_O O_IOPTPLOT_2
Setup Main_O O_IOPTPLOT_3
Setup Main_O O_IOPTPLOT_4
|===OBJECT AND PART COUNT======================================================
ObjectPartCount ---------------------------------------------------------------
|TEMPLATE OBJECTS PARTS RLTS MAXINPUT MAXOUTPUT
EndEnvironmentRefrig 2 2 15 
EndFlowCap 1 2 2 
EngCylGeom 2 0 0 
EngCylHeatTr 1 0 0 
EngCylTWall 1 0 0 
EngCylTWallSoln 1 0 0 
EngineCrankTrain 1 1 134 
FECylinderStructure 1 0 0 
FlowControlExplicit 1 0 0 
FlowSplitGeneral 2 4 94 
FlowSplitTRight 2 4 94 
FluidInitialState 2 0 0 
FluidRefrigerant 1 0 0 
Lookup2D 1 1 5 2 1 
MaterialThermalProp 4 0 0 
MathEquation 3 4 103 3 1 
MonitorSignal 1 1 12 2 0 
MovingAverage 2 8 4 1 1 
ODEControlExplicit 1 0 0 
OrificeConn 3 31 34 
PhTsDiagramRefrig 1 1 0 
PipeRound 10 21 193 
PistonCylinder 1 2 847 
RLTCreator 1 1 12 2 0 
RLTDependenceXY 3 0 0 
RLTScoreboardListDef 8 0 0 
RLTSensor 1 1 12 0 4 
SampledOutput 1 1 2 4 0 
SensorConn 1 9 2 
ValveCamConn 2 8 36 
WallThermalBoundary 2 0 0 
WallThermalProperty 2 0 0 
XYTable 2 0 0 
XYZPoints 1 0 0 
PhantomConn 1 2 0
PhantomControlConn 1 18 0
NameValuePairs ----------------------------------------------------------------
CASE_SETUP_CASE_ON=1   | Number of cases turned on in Case Setup
DOE_CASE_ON=0   | Number of DOE cases (experiments) to be run
CASES=1   | For array allocation. CasesOn x DOE_CASE_ON + totalCases
NMXMAP=0
NMYMAP=0
NMXGMATX=0
NMYGMATX=0
MXMULTPROF=0
NCTMXCYL=2
NGEARMAX=0
AXZONE=0
NSENSORS=9
NACTUATORS=0
NMULTLRDNN=0
TLEMISARR=0
NMAXCHAINLINKS=0
NMAXCHAINLINKSSI=0
NMAXBELTELEMS=0
NMAXBELTELEMSTB=0
NMAXBELTELEMSCVT=0
NMAXBEAMGUIDE=0
NELMAXSOLID2D=0
ELMTYPSOL3D=0
NNDEDGEMAXSOL3D=0
NELMAXSOL3D=0
NELMAXFELB=0
NLOCMAX=2
NEQMXODEQ=0
NINMXODEQ=0
LASTPARTID=66366
MXPIPETABLE=0
NTWALSOLNPARTS=2
NINPSIMUHARN=0
NOUTSIMUHARN=0
SITETABLES=0
NSPRGMAXARCS=0
ORIGINALBUILD=0
ORIGINALVER=70
GTIDEBUG=4
GTSTORE_CHECK=0
RESTART_WRITE=0
RESTART_READ=0
SIM_ID=55d350c9-5391-4036-96b5-fd8249095e94
|===REFERENCE OBJECTS==========================================================
EngCylGeom ---------------------------------------------------------------[21]
|NAME BORE STROKE RODLEN COMPRAT HCLEAR PINOFF STRKFLG JTRUETDC pstiff copy_1_of_pstiff prelod 
 $ cylgeom "[bore]" "[stroke]" "[conrod_length]" "[compression_ratio]" 1.5
 0 2xradius piston-position
 ign ign ign
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ cylgeom_crank "[bore-crank]" "[stroke]" "[conrod_length]" "[compression_ratio]" 1.5
 0 2xradius piston-position
 ign ign ign
EngCylHeatTr -------------------------------------------------------------[30]
|NAME HTRTYP USRHTMOD HTMULT HTMULT1 HTMULT2 HTMULT3 HTMULT4 AHEAD APIST MULTRAD HGFILE JWEIGHT LOSPDENH 
 $ Heat-transfer-cyl WoschniGT ign 0.5 ign ign ign ign 1 1 ign ign hybrid on
|# 830|
EngCylTWall ---------------------------------------------------------------[4]
|NAME THEAD TPIST TCYL 
 $ twall-fromCyl1 head_temp:1&0 piston_temp:1&0 cylinder_temp:1&0
EngCylTWallSoln ---------------------------------------------------------[114]
|NAME FECYLSTRUC TCYCINCR1 TCYCINCR2 TCYCINCR3 ZSHIFT nameFEPN THEAD TPIST1 TCYL1 TVALVE1 TVALVE2 TVALVE3 TVALVE4 TVALVE5 TCOOLCYL HCOOLCYL TCOOLHD HCOOLHD HVSCOOL TOILCYL HOILCYL TOILHEAD HOILHEAD TOILPIST HOILPIST multpistoil TOIL2PIST HOIL2PIST TOIL3PIST HOIL3PIST TAMBCYL HAMBCYL TAMBHEAD HAMBHEAD nameint1 nameint2 nameint3 nameint4 nameint5 nameexh1 nameexh2 nameexh3 nameexh4 nameexh5 nameexh6 nameexh7 nameexh8 nameexh9 nameexh10 
 $ tw1_detailFEM tw1_detailFEM on ign ign on ign
 473.16 473.16 473.16 733.15 733.15 373.15 373.15 def
 366.15 100 366.15 100 def 383.15 100 ign ign 403.15 100 ign ign ign ign ign ign ign ign ign
 ign ign ign ign ign ign ign ign ign ign ign ign ign ign ign
|# 973043|
|@ multipliers applied in HeatTransfer model
FECylinderStructure ------------------------------------------------------[23]
|NAME HSKIRTC HRINGP HRINGC HVALVS HVALVG HGASRE HGASMAT HGASTH RINGFR SKIRTFR RESHDVS HMATL HDECK HDOME AHEADC PLTVALV VSEAT JPPORT0 JPPORT1 JPPORT3 PMATL PDECK PCUPNAME HEIGHT SKIRT RING SKCONT APISTC PISTVOL FEPIST CMATL CTHICK LENGTH COOL1 COOL2 USE2DCYL USE3DCYL THETAWJKT HDWJKTANG THETA2 BETA2 RMESH TMESH ZMESH IMATL XINTHK IINRES JPLTGSKT %15 PORT# SRFDIA THICK XCOORD YCOORD HTMULB VMATL OPENFRC PPTLEN PPTDIAG PPTTHK ivcav SEATREF GUIDEREF jvbangl 
 $ tw1_detailFEM def def def def def 5.0E-5 Head_Gasket_Obsolete def def def def
 Iron 40 0 def on off on ign ign
 Aluminum 43 ign 360 22 15 def def def ign
 iron 36 650 15 450 on ign ign ign ign ign ign ign ign ign ign ign ign
# 4
% 1 88.0 def -46.0 -46.0 def iron def def def ign ign def ign off 
% 2 88.0 def -46.0 46.0 def iron def def def ign ign def ign off 
% 3 88.0 def 46.0 -46.0 def iron def def def ign ign def ign off 
% 4 88.0 def 46.0 46.0 def iron def def def ign ign def ign off 
|# 970207|970212|970226|
FlowControlExplicit ------------------------------------------------------[42]
|NAME TSMAX TSMULT FRM_DT RATIOMXFLOWDT SSTOL TEMPCONV TEMPRATECONV NCYCFLW FLOSS DEFINTRP CFCONS HGCONS ZEROQ UNSTDYMOD CFUNSTDY HGUNSTDY REALGAS VOLVISC MVSOLV PLUGFLOW MOMSOLN 
 $ ExplicitControl def def on def def ign ign 3
 Automatic improved def def off v75_b1 def def GTI_cylinder mass off Off off
|# 972098|
FluidInitialState --------------------------------------------------------[40]
|NAME PRES TEMP FLUID ALT REFALT ALTOPT RELHUM HUMIDPROP ICRH REFP REFT 
 $ intake 1 300 Water
 ign ign ign ign ign on ign ign
|# 964075|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ RefrInit_state "[p_refrig_init]" "[T_refrig_init]" Water
 ign ign ign ign ign on ign ign
|# 964075|
FluidRefrigerant ---------------------------------------------------------[94]
|NAME PREDEFSPEC2 USERFLUID REFMAP ACSC SCMPR FRCTR ALTSOLN NISTver OILFLUIDOBJ OIL_MFRAC HG_METH CF_METH 
 $ Water WATER ign ign
 off ign off off v9.1
 ign ign ign ign
|# 964244|
MaterialThermalProp ------------------------------------------------------[13]
|NAME TCOND COND TRHO RHO TCP CP OPACITY TEMPMIN TEMPMAX RESOLUTION COND1 DENSITY SPHEAT 
 $ Aluminum
TCOND:6:NUM> 100.0 200.0 300.0 400.0 600.0 800.0 <
COND:6:NUM> 302.0 237.0 237.0 240.0 231.0 218.0 <
TRHO:1:NUM> 300.0 <
RHO:1:NUM> 2702.0 <
TCP:6:NUM> 100.0 200.0 300.0 400.0 600.0 800.0 <
CP:6:NUM> 482.0 798.0 903.0 949.0 1033.0 1146.0 <
 opaque def def def ign ign ign
|@ Pure
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ Head_Gasket_Obsolete
TCOND:1:NUM> 300.0 <
COND:1:NUM> 1.234 <
TRHO:2:NUM> 100.0 5000.0 <
RHO:2:NUM> 1.0 1.0 <
TCP:1:NUM> 300.0 <
CP:1:NUM> 2500000.0 <
 opaque def def def ign ign ign
|@ This object created by Evolution.  See Long Comment!!!!
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ Iron
TCOND:9:NUM> 100.0 200.0 300.0 400.0 600.0 800.0 1000.0 1200.0 1500.0 <
COND:9:NUM> 134.0 94.0 80.2 69.5 54.7 43.3 32.8 28.3 32.1 <
TRHO:1:NUM> 300.0 <
RHO:1:NUM> 7870.0 <
TCP:9:NUM> 100.0 200.0 300.0 400.0 600.0 800.0 1000.0 1200.0 1500.0 <
CP:9:NUM> 216.0 384.0 447.0 490.0 574.0 680.0 975.0 609.0 654.0 <
 opaque def def def ign ign ign
|@ Pure
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ iron
TCOND:1:NUM> 300.0 <
COND:1:NUM> 50.0 <
TRHO:2:NUM> 100.0 5000.0 <
RHO:2:NUM> 1.0 1.0 <
TCP:1:NUM> 300.0 <
CP:1:NUM> 3100000.0 <
 opaque def def def ign ign ign
|@ This object created by Evolution.  See Long Comment!!!!
ODEControlExplicit -------------------------------------------------------[23]
|NAME DTMXODE IMXITS TSRLX DYNTSR DYNTSM MAXORD RKACC ABSACC DNORM VNORM RDAN RVACCN HPACCN RKACCEM VNORMEM INORMEM LNORMEM FNORMEM 
 $ Explicit-def def def def def def def
 def def def def def def def
 1.e-6 1.e-3 1.e-3 1.e-3 0.1
|@ Recommended for Runge-Kutta integrator
RLTDependenceXY ----------------------------------------------------------[32]
|NAME RLT1 RLTDINITX RLTDINIT DEPOBJ RLTDIPER RLTHISTPLOT 
 $ cylinder_temp cyl123TW:Cyl-1 300 ign def
 1 off
|# 812423|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ head_temp hd123TW:Cyl-1 300 ign def
 1 off
|# 812423|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ piston_temp pston123TW:Cyl-1 300 ign def
 1 off
|# 812423|
RLTScoreboardListDef ------------------------------------------------------[7]
|NAME RLTScoreL 
 $ Cylinder
RLTScoreL:6> volefcm imepc cylpmx ieffc burnmfcs faefectv <
|@ This list contains the default RLTs displayed in the "Cylinder" Scoreboard
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ Engine
RLTScoreL:5> avgrpm imep bmep volef volefm <
|@ This list contains the default RLTs displayed in the "Engine" Scoreboard
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ HeatExchangers
RLTScoreL:9> favl pavl htav hx-exthtrall hx-inthtrall hx-masext hx-masint hx-intspi hx-piext <
|@ This list contains the default RLTs displayed in the "Heat Exchangers" Scoreboard
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ Injector
RLTScoreL:22> totmnozcp xtotp1 xtotp2 xtotp3 xtotp4 xtotp5 xtotp6 xtotp7 xtotp8 xtotp9 xtotp10 totvnozcp vtotp1 vtotp2 vtotp3 vtotp4 vtotp5 vtotp6 vtotp7 vtotp8 vtotp9 vtotp10 <
|@ This list contains the default RLTs displayed in the "Detailed Injector" Scoreboard
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ Lubrication
RLTScoreL:11> jbrgqavg jbrgfric jbrgftmn jbrgtoil jbrgtris fmr-flrt pmp-pwra pmp-dpa vfr avgpwrs dpavg <
|@ This list contains the default RLTs displayed in the "Lubrication" Scoreboard
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ RefrigFlowMach
RLTScoreL:7> cmp-rpma cmp-prma cmp-prsa pmp-dpa cmp-masa cmp-pwra cmp-effa <
|@ This list contains the default RLTs displayed in the "REFRIG FLOW" Scoreboard
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ Turbo
RLTScoreL:5> cmp-rpma cmp-prma cmp-masa cmp-pwra cmp-effa <
|@ This list contains the default RLTs displayed in the "Turbocharger" Scoreboard
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ Vehicle
RLTScoreL:5> vehispd engrpm output1 output2 output3 <
|@ This list contains the default RLTs displayed in the "Vehicle" Scoreboard
WallThermalBoundary -------------------------------------------------------[8]
|NAME TG HG TRAD FREEC 
 $ exhaust_wall "[exhaust_Temp-out]" 15 "[exhaust_Temp-out]" off
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ intake_wall "[intake_Temp-out]" 15 "[intake_Temp-out]" off
WallThermalProperty -------------------------------------------------------[8]
|NAME %3 EMISS THICK MATNAME 
 $ exhaust_wall
# 1
% 0.8 3.0 Iron 
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ intake_wall
# 1
% 0.8 3.0 Iron 
XYTable ------------------------------------------------------------------[35]
|NAME USER1 USER2 TYPE XSHFT XMULT YSHFT YMULT ILKPTYP SMOOTH JPLTPROF ISTRIP YMIN YMAX 
 $ ent-lower
USER1:4:NUM> 1.0 2.0 3.0 4.0 <
USER2:4:NUM> 6200.0 6200.0 6200.0 6200.0 <
 endpoints def def def def interpolate-linear ign off none ign ign
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ ent-upper
USER1:4:NUM> 1.0 2.0 3.0 4.0 <
USER2:4:NUM> 6900.0 6900.0 6900.0 6900.0 <
 endpoints def def def def interpolate-linear ign off none ign ign
XYZPoints ----------------------------------------------------------------[53]
|NAME TABOUTX TABOUTY XSHFT XMULT YSHFT YMULT ZSHFT ZMULT PLT0 DXDUP DYDUP GRIDEXT NXGRID NYGRID YLOBOUND YHIBOUND IMPRVBND AUTOBOUND ZERRORCHKS ZERRORCHKA ZERRORCHKR PLT1 X Y Z 
 $ h2s-lookup endpoints endpoints def def def def def def on
 def def Proximity def def ent-lower ent-upper on ign on ign ign off
X:35:NUM> 1.0 1.0 1.0 1.0 1.0 1.5 1.5 1.5 1.5 1.5 2.0 2.0 2.0 2.0 2.0 2.5 2.5 2.5 2.5 2.5 3.0 3.0 3.0 3.0 3.0 3.5 3.5 3.5 3.4 4.0 4.0 4.0 4.0 4.0 4.0 <
Y:35:NUM> 6400.0 6500.0 6600.0 6700.0 6800.0 6400.0 6500.0 6600.0 6700.0 6800.0 6400.0 6500.0 6600.0 6700.0 6800.0 6400.0 6500.0 6600.0 6700.0 6800.0 6400.0 6500.0 6600.0 6700.0 6800.0 6400.0 6500.0 6600.0 6700.0 6800.0 6400.0 6500.0 6600.0 6700.0 6800.0 <
Z:35:NUM> 2317500.0 2354800.0 2392100.0 2429400.0 2466600.0 2376700.0 2415100.0 2453600.0 2492000.0 2530500.0 2420300.0 2459600.0 2499000.0 2538300.0 2577600.0 2455100.0 2495200.0 2535300.0 2575300.0 2615400.0 2484300.0 2525000.0 2565600.0 2606300.0 2647000.0 2509400.0 2550600.0 2591800.0 2628000.0 2698300.0 2531600.0 2573200.0 2614900.0 2656600.0 2698300.0 <
|# 3205|966716|
|@ X = pressure (bar); Y = entropy (J/kg-K); Z = enthalpy (J/kg)
|===COMPONENT OBJECTS==========================================================
EndEnvironmentRefrig -----------------------------------------------------[36]
|NAME PRES TEMP TSU QUAL ENTH REFRIG 
 $ discharge "[expander_discharge_Pres]" "[expander_discharge_Temp]" ign ign ign Water
|# 863024|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ suction "[expander_suction_Pres]" "[expander_suction_Temp]" ign ign ign Water
|# 863024|
EngineCrankTrain --------------------------------------------------------[281]
|NAME ENGTYP SPLDOPT RPM FRIC ANGSTRT %2 CYLGEOM CYLCSLD %3 CYLINDER# FINTRVL CYLTYPE2 PTCvolef VOLEFP namrlt namtab ACTUSTRK FILTMOVAVG FILTFIRSTORD FILTQUANT SYSBASOP1 SYSBASOP2 FWINER NCIINR %4 CYLNOAX CYLANG NAXPOS JBEARING 
 $ CrankTrain 2-stroke speed "[expander-rpm]" 0 -20
# 2
% cylgeom ign 
% cylgeom_crank ign 
# 2
% 1 0.0 ign 
% 2 180.0 ign 
 intake suction-line1 ign ign Static on ign ign ign ign
 ign def
# 1
% ign def def on 
|# 974813|
FlowSplitGeneral --------------------------------------------------------[293]
|NAME VOL HTAREA PTCini SMOOTH MATER ROUGH PNUM TWALIMP CALCHEADER HEATG HEATB TWAL THERMPRIM ADIABATIC CHT HEATINP TCRO CONDENSE HGCOLB HGUSER HGACTU HTCold HTCenhanced dlen CFR NOFRIC CFHGUSER ACCELF %9 PORT# ANG IS3D ANGX ANGY ANGZ DX DIAC UserDim 
 $ exh 800000 def RefrInit_state on ign ign def
 ign on exhaust_wall exhaust_wall "[outlet_wall_Temp]" ign ign 1 ign ign off on ign ign on ign ign
 1 ign ign ign
# 3
% 1 ign ign 180.0 90.0 90.0 150.0 128.0 ign 
% 2 ign ign 0.0 90.0 90.0 80.0 90.0 ign 
% 3 ign ign 0.0 90.0 90.0 80.0 90.0 ign 
|# 977513|972556|122|967904|113|971844|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ int 800000 def RefrInit_state on ign ign def
 ign on intake_wall intake_wall "[intake_wall_Temp]" ign ign 1 ign ign off on ign ign on ign ign
 1 ign ign ign
# 3
% 1 ign ign 180.0 90.0 90.0 150.0 128.0 ign 
% 2 ign ign 0.0 90.0 90.0 80.0 90.0 ign 
% 3 ign ign 0.0 90.0 90.0 80.0 90.0 ign 
|# 977513|972556|122|967904|113|971844|
FlowSplitTRight ---------------------------------------------------------[228]
|NAME DIA LENGTH HTAREA PTCini SMOOTH MATER ROUGH PNUM TWALIMP CALCHEADER HEATG HEATB TWAL THERMPRIM ADIABATIC CHT HEATINP TCRO CONDENSE HGCOLB HGUSER HGACTU HTCold HTCenhanced CFR NOFRIC CFHGUSER ACCELF ACC_ANGLE 
 $ evap_turb_T2 130 80 def RefrInit_state on ign ign def
 ign on intake_wall intake_wall "[intake_wall_Temp]" ign ign def ign ign off on ign ign on ign
 def ign ign ign ign
|# 977528|142|972558|971836|968038|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ turb_recup_T2 130 80 def RefrInit_state on ign ign def
 ign on exhaust_wall exhaust_wall "[outlet_wall_Temp]" ign ign def ign ign off on ign ign on ign
 def ign ign ign ign
|# 977528|142|972558|971836|968038|
Lookup2D -----------------------------------------------------------------[30]
|NAME NAMXYZM XLABEL YLABEL ZLABEL OUTLABEL 
 $ h2s h2s-lookup
 "X Input" "Y Input" "Z Input (Reverse Lookups Only)" Output
MathEquation -------------------------------------------------------------[66]
|NAME EQUATION ERRORFLAG VARDESCS VARNAMES SIGNAME TERMNAMES TERMEQUAS OUTLABEL 
 $ eff-isentropic "=(h2a-h1a)/(h2s-h1a)" error_message
VARDESCS:3> suctionenthalpy dischargeenthalpyactual dischargeenthalpyisentropic <
VARNAMES:3> h1a h2a h2s <
SIGNAME:1> ign <
TERMNAMES:1> ign <
TERMEQUAS:1> ign <
 Output
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ enth-static "=htot-.5*v^2" error_message
VARDESCS:2> totalenthalpy velocity <
VARNAMES:2> htot v <
SIGNAME:1> ign <
TERMNAMES:1> ign <
TERMEQUAS:1> ign <
 Output
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ Pr "=p1t/p2t" error_message
VARDESCS:2> suctionpressuretotal dischargepressuretotal <
VARNAMES:2> p1t p2t <
SIGNAME:1> ign <
TERMNAMES:1> ign <
TERMEQUAS:1> ign <
 Output
MonitorSignal ------------------------------------------------------------[42]
|NAME XAXISTYPE SCRL XMAX YLABEL YMIN YMAX YLAB2 YMIN2 YMAX2 YRESCALE LINEWID DISPLAY REFCURVE PREVCASE TITLE %4 YLEG YSIG YAXIS DISPLAYCURV 
 $ Turbine_power time off def "Turbine power, kW" 0 300 "isoentropic efficiency" 0.7 1.1 off 2 show ign def ign
# 2
% "Turbine power" ign Y1 show 
% efficiency ign Y2 show 
MovingAverage ------------------------------------------------------------[27]
|NAME CYWIDTH MAXCYTMWIDTH TMWIDTH TSWIDTH RSWIDTH YINIT NINTVLS INLABEL OUTLABEL 
 $ Avg 1 ign ign ign ign 1 20
 Input Output
|# 978407|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ Avg-h2 1 ign ign ign ign 2 7
 Input Output
|# 978407|
PhTsDiagramRefrig --------------------------------------------------------[42]
|NAME PNAME XLOC TPLTFREQ TPLTNF 
 $ Ph_diag
PNAME:2> suction-line1 discharge-line-1 <
XLOC:2> ign ign <
 1 def
PipeRound ---------------------------------------------------------------[381]
|NAME D1 D2 PIPEL DXP PTCini SMOOTH MATER ROUGH RBENDD ABENDD ELEV PNUM TWALIMP CALCHEADER HEATG HEATB TWAL THERMPRIM ADIABATIC CHT HEATINP TCRO HGCOLB HGUSER HGACTU CONDENSE CFR NOFRIC CFHGUSER ACCELF CP1AUTO cp1zero CP1 CP2 
 $ discharge-line-3 130 def 80 "[dx]" RefrInit_state on ign ign ign ign ign def
 ign on exhaust_wall exhaust_wall "[outlet_wall_Temp]" ign ign def ign ign on ign ign off
 def ign ign ign on ign ign ign
|# 972469|176|967955|967960|971852|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ evap_turb 130 def 150 "[dx]" RefrInit_state on ign ign ign ign ign def
 ign on intake_wall intake_wall "[intake_wall_Temp]" ign ign def ign ign on ign ign off
 def ign ign ign on ign ign ign
|# 972469|176|967955|967960|971852|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ evap_turb_2 130 def 160 "[dx]" RefrInit_state on ign ign ign ign ign def
 ign on intake_wall intake_wall "[intake_wall_Temp]" ign ign def ign ign on ign ign off
 def ign ign ign on ign ign ign
|# 972469|176|967955|967960|971852|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ exhaust-port 128 def 80 "[dx]" RefrInit_state on ign ign ign ign ign def
 ign on exhaust_wall exhaust_wall "[outlet_wall_Temp]" ign ign def ign ign on ign ign off
 def ign ign ign on ign ign ign
|# 972469|176|967955|967960|971852|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ intake-port 128 def 50 "[dx]" RefrInit_state on ign ign ign ign ign def
 ign on intake_wall intake_wall "[intake_wall_Temp]" ign ign def ign ign on ign ign off
 def ign ign ign on ign ign ign
|# 972469|176|967955|967960|971852|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ p761 90 90 150 "[dx]" RefrInit_state on ign ign ign ign ign 1
 ign on intake_wall intake_wall "[intake_wall_Temp]" ign ign 1 ign ign on ign ign off
 1 ign ign ign on ign ign ign
|# 972469|176|967955|967960|971852|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ p762 90 90 150 "[dx]" RefrInit_state on ign ign ign ign ign 1
 ign on exhaust_wall exhaust_wall "[outlet_wall_Temp]" ign ign 1 ign ign on ign ign off
 1 ign ign ign on ign ign ign
|# 972469|176|967955|967960|971852|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ suction-line1 130 def 100 "[dx]" RefrInit_state on ign ign ign ign ign def
 ign on intake_wall intake_wall "[intake_wall_Temp]" ign ign def ign ign on ign ign off
 def ign ign ign on ign ign ign
|# 972469|176|967955|967960|971852|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ turb_recup 130 def 160 "[dx]" RefrInit_state on ign ign ign ign ign def
 ign on exhaust_wall exhaust_wall "[outlet_wall_Temp]" ign ign def ign ign on ign ign off
 def ign ign ign on ign ign ign
|# 972469|176|967955|967960|971852|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ turb_recup_2 130 def 160 "[dx]" RefrInit_state on ign ign ign ign ign def
 ign on exhaust_wall exhaust_wall "[outlet_wall_Temp]" ign ign def ign ign on ign ign off
 def ign ign ign on ign ign ign
|# 972469|176|967955|967960|971852|
PistonCylinder -----------------------------------------------------------[57]
|NAME PTCini TWAL TWALCPL HEATTR FLOW PTSCALBF 
 $ Cylinder RefrInit_state tw1_detailFEM ign Heat-transfer-cyl ign on
|# 952348|
RLTCreator ---------------------------------------------------------------[26]
|NAME %6 Label YSIG AVGTYP UNIT MULT VATANGLE 
 $ Expander-Perf
# 2
% IsentropicEfficiency ign instantaneous 265 def def 
% PressureRatio ign instantaneous 265 def def 
RLTSensor ----------------------------------------------------------------[18]
|NAME %3 RLTNAME Y0 YGAIN IOPTYPE IOPLEN 
 $ Results
# 4
% airflow:CrankTrain-1:81:79 ign def 
% bkw:CrankTrain-1 ign def 
% userrlt01:Expander-Perf ign def 
% userrlt02:Expander-Perf ign def 
 first_update ign
SampledOutput ------------------------------------------------------------[59]
|NAME PLOTX SAMMAXPLOT FILENAME FILEPCASE TXTTIME TXTCYCANG TXTCUMANG TXTTSTEP TXTTRPOS CHEADER PRECISION SCREENNew LSTCYC LSTCYFTDC ENTRUN SPECINT WINSSTYPE WINSTART WINEND CTRLSIGNAL SAMTYPE SAMRATE %4 SIGLABEL YSIG SIGUNIT OUTLABEL 
 $ output_results cycle_angle def def off off on off off off def single_precision ign
 on ign ign ign ign ign ign ign
 cycles 1
# 4
% steam_MFR ign 79 ign 
% expander_power ign 104 ign 
% isentropic_efficiency ign 0 ign 
% pressure_ratio ign 0 ign 
|# 966087|355131|971507|
|===CONNECTION OBJECTS=========================================================
OrificeConn -------------------------------------------------------------[273]
|NAME DIA ALORF PWLORF ONUM CD1 CD2 PLUG RCRAD ENDCOR1 ENDCOR2 HEATCC MFLOWI PRESREC CLAMMLT 
 $ bellmouth def ign ign def 1 1 def ign
 def def def def PressureRecovery def
|# 617|
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ no_heat def ign ign def def def def ign
 def def ign def PressureRecovery def
|# 617|
ValveCamConn -------------------------------------------------------------[95]
|NAME VTMNG VTMNGREF VTMNGANC ATTCYL CMPCAM DRVREF HEATCC VLASH VALSHAPE NOMLIFT VDWELLMAXLF VSTRAN ANCHORSTR VSTRLF THET LIFT VDIA CDAREF LIFTUNIT AMULT ONUM SWRLMULT TMBMULT L/DI CD11 CD22 CSWL CTMB INTEXH EHEIGHT EHEIGHT2 EFLAG PLOTFLAG 
 $ valconexh "[EVO]" TDCFiring openingRLT on ign ign ign
 0.4 ign ign ign "[EV_length]" ign 1
THET:167:NUM> -83.0 -82.0 -81.0 -80.0 -79.0 -78.0 -77.0 -76.0 -75.0 -74.0 -73.0 -72.0 -71.0 -70.0 -69.0 -68.0 -67.0 -66.0 -65.0 -64.0 -63.0 -62.0 -61.0 -60.0 -59.0 -58.0 -57.0 -56.0 -55.0 -54.0 -53.0 -52.0 -51.0 -50.0 -49.0 -48.0 -47.0 -46.0 -45.0 -44.0 -43.0 -42.0 -41.0 -40.0 -39.0 -38.0 -37.0 -36.0 -35.0 -34.0 -33.0 -32.0 -31.0 -30.0 -29.0 -28.0 -27.0 -26.0 -25.0 -24.0 -23.0 -22.0 -21.0 -20.0 -19.0 -18.0 -17.0 -16.0 -15.0 -14.0 -13.0 -12.0 -11.0 -10.0 -9.0 -8.0 -7.0 -6.0 -5.0 -4.0 -3.0 -2.0 -1.0 0.0 1.0 2.0 3.0 4.0 5.0 6.0 7.0 8.0 9.0 10.0 11.0 12.0 13.0 14.0 15.0 16.0 17.0 18.0 19.0 20.0 21.0 22.0 23.0 24.0 25.0 26.0 27.0 28.0 29.0 30.0 31.0 32.0 33.0 34.0 35.0 36.0 37.0 38.0 39.0 40.0 41.0 42.0 43.0 44.0 45.0 46.0 47.0 48.0 49.0 50.0 51.0 52.0 53.0 54.0 55.0 56.0 57.0 58.0 59.0 60.0 61.0 62.0 63.0 64.0 65.0 66.0 67.0 68.0 69.0 70.0 71.0 72.0 73.0 74.0 75.0 76.0 77.0 78.0 79.0 80.0 81.0 82.0 83.0 <
LIFT:167:NUM> 0.0 0.002007502 0.007847507 0.017885016 0.031755029 0.049457545 0.071357564 0.097090088 0.126655114 0.160417645 0.195640177 0.230680208 0.26590274 0.301125272 0.336347803 0.371570335 0.406792867 0.441832899 0.47705543 0.512277962 0.547500494 0.582175525 0.62050056 0.666125601 0.724525654 0.801175723 0.903375815 1.025650925 1.180776065 1.36327623 1.574976421 1.815876638 2.082326879 2.372502141 2.684577422 3.013077719 3.359828031 3.717528354 4.086178687 4.460304024 4.841729368 5.224979714 5.60823006 5.991480406 6.37290575 6.750681091 7.122981427 7.487981756 7.84750708 8.199732398 8.542832708 8.878633011 9.203483304 9.52103359 9.827633867 10.12510914 10.41163439 10.68903464 10.95548488 11.21281012 11.45918534 11.69461055 11.92091076 12.13626095 12.34066113 12.53411131 12.71843648 12.89181163 13.05423678 13.20571191 13.34806204 13.47946216 13.59991227 13.70941237 13.80978746 13.89921254 13.97768761 14.04521267 14.10361272 14.15106277 14.1875628 14.21311282 14.22953784 14.23501284 14.22953784 14.21311282 14.1875628 14.15106277 14.10361272 14.04521267 13.97768761 13.89921254 13.80978746 13.70941237 13.59991227 13.47946216 13.34806204 13.20571191 13.05423678 12.89181163 12.71843648 12.53411131 12.34066113 12.13626095 11.92091076 11.69461055 11.45918534 11.21281012 10.95548488 10.68903464 10.41163439 10.12510914 9.827633867 9.52103359 9.203483304 8.878633011 8.542832708 8.199732398 7.84750708 7.487981756 7.122981427 6.750681091 6.37290575 5.991480406 5.60823006 5.224979714 4.841729368 4.460304024
4.086178687 
3.717528354 3.359828031 3.013077719 2.684577422 2.372502141 2.082326879 1.815876638 1.574976421 1.36327623 1.180776065 1.025650925 0.903375815 0.801175723 0.724525654 0.666125601 0.62050056 0.582175525 0.547500494 0.512277962 0.47705543 0.441832899 0.406792867 0.371570335 0.336347803 0.301125272 0.26590274 0.230680208 0.195640177 0.160417645 0.126655114 0.097090088 0.071357564 0.049457545 0.031755029 0.017885016 0.007847507 0.002007502 0.0 <
 88 constant LiftOverDiam 1. def ign ign
L/DI:17:NUM> 0.0 0.017 0.033 0.05 0.067 0.083 0.1 0.117 0.133 0.15 0.167 0.183 0.2 0.217 0.233 0.25 0.28 <
CD11:17:NUM> 0.0 0.039548387 0.086709677 0.140129032 0.198451613 0.25516129 0.303043057 0.337184174 0.365174471 0.392148663 0.410072749 0.422967742 0.440955557 0.448467958 0.45415137 0.459584143 0.463 <
CD22:17:NUM> 0.0 0.039548387 0.086709677 0.140129032 0.198451613 0.25516129 0.303043057 0.337184174 0.365174471 0.392148663 0.410072749 0.422967742 0.440955557 0.448467958 0.45415137 0.459584143 0.463 <
CSWL:1> ign <
CTMB:1> ign <
 automatic 1 1 valve on
|# 972165|
|@ nova_vacka-vyfukova
|++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 $ valconint "[IVO]" TDCFiring openingRLT on ign ign ign
 0.4 ign ign ign "[IV_length]" ign 1
THET:167:NUM> -83.0 -82.0 -81.0 -80.0 -79.0 -78.0 -77.0 -76.0 -75.0 -74.0 -73.0 -72.0 -71.0 -70.0 -69.0 -68.0 -67.0 -66.0 -65.0 -64.0 -63.0 -62.0 -61.0 -60.0 -59.0 -58.0 -57.0 -56.0 -55.0 -54.0 -53.0 -52.0 -51.0 -50.0 -49.0 -48.0 -47.0 -46.0 -45.0 -44.0 -43.0 -42.0 -41.0 -40.0 -39.0 -38.0 -37.0 -36.0 -35.0 -34.0 -33.0 -32.0 -31.0 -30.0 -29.0 -28.0 -27.0 -26.0 -25.0 -24.0 -23.0 -22.0 -21.0 -20.0 -19.0 -18.0 -17.0 -16.0 -15.0 -14.0 -13.0 -12.0 -11.0 -10.0 -9.0 -8.0 -7.0 -6.0 -5.0 -4.0 -3.0 -2.0 -1.0 0.0 1.0 2.0 3.0 4.0 5.0 6.0 7.0 8.0 9.0 10.0 11.0 12.0 13.0 14.0 15.0 16.0 17.0 18.0 19.0 20.0 21.0 22.0 23.0 24.0 25.0 26.0 27.0 28.0 29.0 30.0 31.0 32.0 33.0 34.0 35.0 36.0 37.0 38.0 39.0 40.0 41.0 42.0 43.0 44.0 45.0 46.0 47.0 48.0 49.0 50.0 51.0 52.0 53.0 54.0 55.0 56.0 57.0 58.0 59.0 60.0 61.0 62.0 63.0 64.0 65.0 66.0 67.0 68.0 69.0 70.0 71.0 72.0 73.0 74.0 75.0 76.0 77.0 78.0 79.0 80.0 81.0 82.0 83.0 <
LIFT:167:NUM> 0.0 0.002007502 0.007847507 0.017885016 0.031755029 0.049457545 0.071357564 0.097090088 0.126655114 0.160417645 0.195640177 0.230680208 0.26590274 0.301125272 0.336347803 0.371570335 0.406792867 0.441832899 0.47705543 0.512277962 0.547500494 0.582175525 0.62050056 0.666125601 0.724525654 0.801175723 0.903375815 1.025650925 1.180776065 1.36327623 1.574976421 1.815876638 2.082326879 2.372502141 2.684577422 3.013077719 3.359828031 3.717528354 4.086178687 4.460304024 4.841729368 5.224979714 5.60823006 5.991480406 6.37290575 6.750681091 7.122981427 7.487981756 7.84750708 8.199732398 8.542832708 8.878633011 9.203483304 9.52103359 9.827633867 10.12510914 10.41163439 10.68903464 10.95548488 11.21281012 11.45918534 11.69461055 11.92091076 12.13626095 12.34066113 12.53411131 12.71843648 12.89181163 13.05423678 13.20571191 13.34806204 13.47946216 13.59991227 13.70941237 13.80978746 13.89921254 13.97768761 14.04521267 14.10361272 14.15106277 14.1875628 14.21311282 14.22953784 14.23501284 14.22953784 14.21311282 14.1875628 14.15106277 14.10361272 14.04521267 13.97768761 13.89921254 13.80978746 13.70941237 13.59991227 13.47946216 13.34806204 13.20571191 13.05423678 12.89181163 12.71843648 12.53411131 12.34066113 12.13626095 11.92091076 11.69461055 11.45918534 11.21281012 10.95548488 10.68903464 10.41163439 10.12510914 9.827633867 9.52103359 9.203483304 8.878633011 8.542832708 8.199732398 7.84750708 7.487981756 7.122981427 6.750681091 6.37290575 5.991480406 5.60823006 5.224979714 4.841729368 4.460304024
4.086178687 
3.717528354 3.359828031 3.013077719 2.684577422 2.372502141 2.082326879 1.815876638 1.574976421 1.36327623 1.180776065 1.025650925 0.903375815 0.801175723 0.724525654 0.666125601 0.62050056 0.582175525 0.547500494 0.512277962 0.47705543 0.441832899 0.406792867 0.371570335 0.336347803 0.301125272 0.26590274 0.230680208 0.195640177 0.160417645 0.126655114 0.097090088 0.071357564 0.049457545 0.031755029 0.017885016 0.007847507 0.002007502 0.0 <
 88 constant LiftOverDiam 1. def ign ign
L/DI:17:NUM> 0.0 0.016 0.032 0.048 0.065 0.081 0.097 0.113 0.129 0.145 0.161 0.177 0.194 0.21 0.226 0.242 0.28 <
CD11:17:NUM> 0.0 0.057419355 0.11622131 0.170942177 0.222878574 0.270819865 0.314160728 0.351690526 0.387404366 0.412827778 0.437887998 0.460950664 0.475780987 0.488795353 0.498783121 0.506652273 0.514 <
CD22:17:NUM> 0.0 0.057419355 0.11622131 0.170942177 0.222878574 0.270819865 0.314160728 0.351690526 0.387404366 0.412827778 0.437887998 0.460950664 0.475780987 0.488795353 0.498783121 0.506652273 0.514 <
CSWL:1> ign <
CTMB:1> ign <
 automatic 1 1 valve on
|# 972165|
|@ nová_vacka-saci
|===CIRCUITS INFO==============================================================
CircuitsList ------------------------------------------------------------------
|CIRCUIT# CATEGORY
0 Breaker
1 Flow
2 Mechanical
3 Control
4 Control
|===PARTS MAP==================================================================
PartsList ---------------------------------------------------------------------
|PART# GEODATA TEMPLATE OBJECT NAME CIRCUITS OVERRIDES
66219 013026004004 EndFlowCap def 59 {1}
66220 039026004004 EndFlowCap def 78 {1}
66189 006015004004 MovingAverage Avg Avg-1 {3}
66171 006007004004 MovingAverage Avg Avg-2 {3}
66184 006017004004 MovingAverage Avg Avg-3 {3}
66199 006005004004 MovingAverage Avg-h2 Avg-4 {3}
66173 006021004004 MovingAverage Avg Avg-5 {3}
66186 006001004004 MovingAverage Avg Avg-6 {3}
66193 006019004004 MovingAverage Avg Avg-7 {3}
66174 006003004004 MovingAverage Avg Avg-8 {3}
66266 040031161021 EngineCrankTrain CrankTrain CrankTrain-1 {2}
66102 026015013013 PistonCylinder Cylinder Cyl-1 {1}
66264 026024013013 PistonCylinder Cylinder Cyl-3 {1} TWAL=twall-fromCyl1
66234 074013004004 EndEnvironmentRefrig discharge discharge-2 {1}
66164 072011004004 PipeRound discharge-line-3 discharge-line-1 {1}
66192 019012018016 RLTCreator Expander-Perf Expander-Perf {3}
65894 009012004004 MonitorSignal Turbine_power Expander-power {3}
66177 010011004004 MathEquation eff-isentropic eff-isen {3}
66188 010004004004 MathEquation enth-static enth-static-1 {3}
66202 010018004004 MathEquation enth-static enth-static-2 {3}
65807 011011004004 PipeRound evap_turb evap_turb-1 {1}
66129 013013004004 PipeRound evap_turb_2 evap_turb_2-1 {1}
66130 013019004004 PipeRound evap_turb_2 evap_turb_2-2 {1}
66128 013015004004 FlowSplitTRight evap_turb_T2 evap_turb_T2-1 {1}
66218 013024004004 FlowSplitTRight evap_turb_T2 evap_turb_T2-3 {1}
66254 037015004004 PipeRound exhaust-port exhaust-port-1 {1}
66255 037024004004 PipeRound exhaust-port exhaust-port-2 {1}
66197 006011004004 Lookup2D h2s h2s {3}
66246 015015004004 PipeRound intake-port intake-port-1 {1}
66247 015024004004 PipeRound intake-port intake-port-2 {1}
66344 016040015032 SampledOutput output_results output_results-1 {4}
66244 077021045030 PhTsDiagramRefrig Ph_diag P-h_diagram {-1}
66169 012013004004 MathEquation Pr Pr {3}
66271 021013004004 PipeRound p761 R201 {1}
|@ Ansaugkanal kurz im Zylinderkopf Zylinder 1
66273 021017004004 PipeRound p761 R201_1 {1}
|@ Ansaugkanal kurz im Zylinderkopf Zylinder 1
66287 021026004004 PipeRound p761 R201_2 {1}
|@ Ansaugkanal kurz im Zylinderkopf Zylinder 1
66295 031013004004 PipeRound p762 R201_3 {1}
|@ Ansaugkanal kurz im Zylinderkopf Zylinder 1
66308 031022004004 PipeRound p762 R201_4 {1}
|@ Ansaugkanal kurz im Zylinderkopf Zylinder 1
66282 021022004004 PipeRound p761 R202 {1}
|@ Ansaugkanal kurz im Zylinderkopf Zylinder 1
66290 031017004004 PipeRound p762 R203 {1}
|@ Ansaugkanal kurz im Zylinderkopf Zylinder 1
66309 031026004004 PipeRound p762 R204 {1}
|@ Ansaugkanal kurz im Zylinderkopf Zylinder 1
66345 009040012030 RLTSensor Results Results-1 {4}
66274 017015004004 FlowSplitGeneral int s536-1 {1}
66286 017024004004 FlowSplitGeneral int s536-2 {1}
66294 035015004004 FlowSplitGeneral exh s536-3 {1}
66304 035024004004 FlowSplitGeneral exh s536-4 {1}
66232 006003004004 EndEnvironmentRefrig suction suction-2 {1}
66205 011003004004 PipeRound suction-line1 suction-line1 {1}
65826 069008004004 PipeRound turb_recup turb_recup-1 {1}
66110 056008004004 PipeRound turb_recup turb_recup-2 {1}
66126 039013004004 PipeRound turb_recup_2 turb_recup_2-1 {1}
66127 039019004004 PipeRound turb_recup_2 turb_recup_2-2 {1}
66134 039015004004 FlowSplitTRight turb_recup_T2 turb_recup_T2-1 {1}
66215 039024004004 FlowSplitTRight turb_recup_T2 turb_recup_T2-3 {1}
SystemMap ---------------------------------------------------------------------
|PART# GEODATA TEMPLATE OBJECT CMP1 CMP2 NAME CIRCUITS OVERRIDES
66213 011007001001 OrificeConn def 66205.2 65807.1 1 {1}
66214 072008001001 OrificeConn def 65826.2 66164.1 2 {1}
66223 013022001001 OrificeConn def 66130.2 66218.1 3 {1}
66224 013025001001 OrificeConn def 66218.2 66219.1 4 {1}
66225 039025001001 OrificeConn def 66220.1 66215.1 5 {1}
66226 039022001001 OrificeConn def 66215.2 66127.1 6 {1}
66346 013011001001 OrificeConn def 65807.2 66129.1 7 {1}
66212 009003001001 OrificeConn def 66232.1 66205.1 8 {1}
66280 016015001001 OrificeConn def 66246.2 66274.1 12 {1}
66288 016024001001 OrificeConn def 66247.2 66286.1 13 {1}
66303 036015001001 OrificeConn def 66294.1 66254.1 14 {1}
66311 036024001001 OrificeConn def 66304.1 66255.1 15 {1}
66245 072013004004 OrificeConn bellmouth 66164.2 66234.1 16 {1}
66250 014015001001 OrificeConn def 66128.3 66246.1 17 {1}
66251 014024001001 OrificeConn def 66218.3 66247.1 18 {1}
66258 038015001001 OrificeConn def 66254.2 66134.3 21 {1}
66259 038024001001 OrificeConn def 66255.2 66215.3 22 {1}
65895 009020004004 SensorConn def 66266.7 65894.1 34 {3} unitDef1=104 unitUsr1=104 unitDef2=0 unitUsr2=0
|![(180,620)][]
66153 068008001001 OrificeConn def 66110.2 65826.1 87 {1}
66132 013014001001 OrificeConn def 66129.2 66128.1 94 {1}
66133 013017001001 OrificeConn def 66128.2 66130.1 95 {1}
66135 039017001001 OrificeConn def 66127.2 66134.1 96 {1}
66136 039014001001 OrificeConn def 66134.2 66126.1 97 {1}
66137 039008001001 OrificeConn def 66126.2 66110.1 98 {1}
66275 019013004004 OrificeConn no_heat 66274.2 66271.1 C201 {1}
66272 019017004004 OrificeConn no_heat 66274.3 66273.1 C201_1 {1}
66284 019026004004 OrificeConn no_heat 66286.3 66287.1 C201_2 {1}
66292 033013004004 OrificeConn no_heat 66295.2 66294.2 C201_3 {1}
66305 033022004004 OrificeConn no_heat 66308.2 66304.2 C201_4 {1}
66281 019022004004 OrificeConn no_heat 66286.2 66282.1 C202 {1}
66289 033017004004 OrificeConn no_heat 66290.2 66294.3 C203 {1}
66306 033026004004 OrificeConn no_heat 66309.2 66304.3 C204 {1}
66276 023013004004 ValveCamConn valconint 66271.2 66102.1 E201 {1}
66277 023017004004 ValveCamConn valconint 66273.2 66102.2 E201_1 {1}
|@ Einla??ventil F??llungskanal Zylinder 1
66283 023026004004 ValveCamConn valconint 66287.2 66264.2 E201_2 {1}
|@ Einla??ventil F??llungskanal Zylinder 1
66291 029013004004 ValveCamConn valconexh 66102.3 66295.1 E201_3 {1}
|@ Einla??ventil F??llungskanal Zylinder 1
66310 029022004004 ValveCamConn valconexh 66264.3 66308.1 E201_4 {1}
|@ Einla??ventil F??llungskanal Zylinder 1
66285 023022004004 ValveCamConn valconint 66282.2 66264.1 E202 {1}
66293 029017004004 ValveCamConn valconexh 66102.4 66290.1 E203 {1}
66307 029026004004 ValveCamConn valconexh 66264.4 66309.1 E204 {1}
66165 080003004004 SensorConn def 66205.14 66199.1 h1a {3} SENSLOC=0 INTERPOLATE=interpolate-linear unitDef1=150 unitUsr1=150 unitDef2=0 unitUsr2=0
66208 079011004004 SensorConn def 65826.14 66184.1 h2a {3} SENSLOC=0 INTERPOLATE=interpolate-linear unitDef1=150 unitUsr1=150 unitDef2=0 unitUsr2=0
66207 078003004004 SensorConn def 66205.20 66186.1 p1t {3} SENSLOC=0 INTERPOLATE=interpolate-linear unitDef1=25 unitUsr1=25 unitDef2=0 unitUsr2=0
66211 080011004004 SensorConn def 65826.1 66189.1 p2 {3} SENSLOC=0 INTERPOLATE=interpolate-linear unitDef1=25 unitUsr1=25 unitDef2=0 unitUsr2=0
66166 077011004004 SensorConn def 65826.20 66173.1 p2t {3} SENSLOC=0 INTERPOLATE=interpolate-linear unitDef1=25 unitUsr1=25 unitDef2=0 unitUsr2=0
66167 079003004004 SensorConn def 66205.25 66171.1 s1 {3} SENSLOC=0 INTERPOLATE=interpolate-linear unitDef1=130 unitUsr1=130 unitDef2=0 unitUsr2=0
66162 077003004004 SensorConn def 66205.17 66174.1 v1 {3} SENSLOC=0 INTERPOLATE=interpolate-linear unitDef1=41 unitUsr1=41 unitDef2=0 unitUsr2=0
66209 078011004004 SensorConn def 65826.17 66193.1 v2 {3} SENSLOC=0 INTERPOLATE=interpolate-linear unitDef1=41 unitUsr1=41 unitDef2=0 unitUsr2=0
66347 001001001001 PhantomConn def 66102.1 66266.1 66347 {0} 
66348 001001001001 PhantomConn def 66264.1 66266.2 66348 {0} 
66349 001001001001 PhantomControlConn def 66173.1 66169.2 66349 {3} 
|![(240,420)][]
66350 001001001001 PhantomControlConn def 66197.1 66177.3 66350 {3} 
66351 001001001001 PhantomControlConn def 66184.1 66202.1 66351 {3} 
66352 001001001001 PhantomControlConn def 66199.1 66188.1 66352 {3} 
66353 001001001001 PhantomControlConn def 66189.1 66197.1 66353 {3} 
66354 001001001001 PhantomControlConn def 66202.1 66177.2 66354 {3} 
66355 001001001001 PhantomControlConn def 66171.1 66197.2 66355 {3} 
66356 001001001001 PhantomControlConn def 66188.1 66177.1 66356 {3} 
66357 001001001001 PhantomControlConn def 66169.1 66192.2 66357 {3} 
66358 001001001001 PhantomControlConn def 66174.1 66188.2 66358 {3} 
66359 001001001001 PhantomControlConn def 66193.1 66202.2 66359 {3} 
66360 001001001001 PhantomControlConn def 66177.1 66192.1 66360 {3} 
66361 001001001001 PhantomControlConn def 66186.1 66169.1 66361 {3} 
|![(240,20)][]
66362 001001001001 PhantomControlConn def 66177.1 65894.2 66362 {3} 
|![(180,120)][]
66363 001001001001 PhantomControlConn def 66345.1 66344.1 66363 {4} 
66364 001001001001 PhantomControlConn def 66345.2 66344.2 66364 {4} 
66365 001001001001 PhantomControlConn def 66345.3 66344.3 66365 {4} 
66366 001001001001 PhantomControlConn def 66345.4 66344.4 66366 {4} 
|===CASE SPECIFICATIONS========================================================
Parameter_Constants -----------------------------------------------------------
bore=351 unitDef=3 unitUser=3 label="Bore"
bore-crank=349.5 unitDef=3 unitUser=3 label="Bore"
compression_ratio=11 unitDef=0 unitUser=0 label="Compression Ratio"
conrod_length=813 unitDef=3 unitUser=3 label="Connecting Rod Length"
dx=80 unitDef=3 unitUser=3 label="Discretization Length"
EV_length=0.98 unitDef=0 unitUser=0 label="Angle Multiplier"
EVO=140 unitDef=179 unitUser=179 label="Cam Timing Angle"
exhaust_Temp-out=373.15 unitDef=32 unitUser=34 label="External Convection Temperature"
expander-rpm=250 unitDef=139 unitUser=139 label="Engine Speed"
expander_discharge_Pres=0.5 unitDef=25 unitUser=25 label="Expander Suction Pressure"
expander_discharge_Temp=354.45 unitDef=32 unitUser=34 label="Expander Suction Temperature"
expander_suction_Pres=20 unitDef=25 unitUser=25 label="Expander Discharge Pressure"
expander_suction_Temp=741.55 unitDef=32 unitUser=34 label="Expander Discharge Temperature"
HTSS=steady unitDef=0 unitUser=0 label="Wall Temperature Solver"
intake_Temp-out=673.15 unitDef=32 unitUser=34 label="External Convection Temperature"
intake_wall_Temp=673.15 unitDef=32 unitUser=34 label="intake pipes Wall Temperature"
IV_length=0.2225 unitDef=0 unitUser=0 label="Angle Multiplier"
IVO=-0.5 unitDef=179 unitUser=179 label="Cam Timing Angle"
outlet_wall_Temp=373.15 unitDef=32 unitUser=34 label="outlet pipes Wall Temperature"
p_refrig_init=20 unitDef=25 unitUser=25 label="Pressure (Absolute)"
stroke=521 unitDef=3 unitUser=3 label="Stroke"
T_refrig_init=741.55 unitDef=32 unitUser=34 label="Refrigerant Initial Temperature"
End ---------------------------------------------------------------------------
Parameters --------------------------------------------------------------------
orig
End ---------------------------------------------------------------------------
|===SUBASSEMBLY SPECIFICATIONS=================================================
<?xml version="1.0" encoding="ISO-8859-1"?>
<subassembly-extension>
    <main>
        <part id="66284"/>
        <part id="66273"/>
        <part id="66308"/>
        <part id="66135"/>
        <part id="66251"/>
        <part id="66205"/>
        <part id="66286"/>
        <part id="66275"/>
        <part id="65894"/>
        <part id="66102"/>
        <part id="66310"/>
        <part id="66264"/>
        <part id="66137"/>
        <part id="66345"/>
        <part id="66218"/>
        <part id="66126"/>
        <part id="66207"/>
        <part id="66288"/>
        <part id="65826"/>
        <part id="66277"/>
        <part id="66266"/>
        <part id="66220"/>
        <part id="66255"/>
        <part id="66128"/>
        <part id="66209"/>
        <part id="66290"/>
        <part id="66244"/>
        <part id="66303"/>
        <part id="66130"/>
        <part id="66211"/>
        <part id="66292"/>
        <part id="66165"/>
        <part id="66246"/>
        <part id="66281"/>
        <part id="66224"/>
        <part id="66305"/>
        <part id="66259"/>
        <part id="66132"/>
        <part id="66213"/>
        <part id="66294"/>
        <part id="66167"/>
        <part id="66283"/>
        <part id="66110"/>
        <part id="66272"/>
        <part id="66226"/>
        <part id="66307"/>
        <part id="66134"/>
        <part id="66215"/>
        <part id="66250"/>
        <part id="66285"/>
        <part id="66274"/>
        <part id="66309"/>
        <part id="66136"/>
        <part id="66344"/>
        <part id="66287"/>
        <part id="66276"/>
        <part id="65895"/>
        <part id="66311"/>
        <part id="66346"/>
        <part id="66219"/>
        <part id="66254"/>
        <part id="66127"/>
        <part id="66208"/>
        <part id="66289"/>
        <part id="66162"/>
        <part id="66232"/>
        <part id="66129"/>
        <part id="66291"/>
        <part id="66164"/>
        <part id="66245"/>
        <part id="66280"/>
        <part id="66153"/>
        <part id="66234"/>
        <part id="65807"/>
        <part id="66223"/>
        <part id="66304"/>
        <part id="66258"/>
        <part id="66212"/>
        <part id="66293"/>
        <part id="66166"/>
        <part id="66247"/>
        <part id="66282"/>
        <part id="66271"/>
        <part id="66225"/>
        <part id="66306"/>
        <part id="66133"/>
        <part id="66214"/>
        <part id="66295"/>
    </main>
    <sa-component center_x="1580" center_y="140" id="66168" name="Pr_and_Eff" sa_id="10" size_x="96" size_y="80"/>
    <subassembly id="10" level="2" name="Pr_and_Eff" pa_id="0" size_x="1000" size_y="1000">
        <part id="66174"/>
        <part id="66186"/>
        <part id="66197"/>
        <part id="66177"/>
        <part id="66188"/>
        <part id="66199"/>
        <part id="66189"/>
        <part id="66169"/>
        <part id="66202"/>
        <part id="66171"/>
        <part id="66192"/>
        <part id="66193"/>
        <part id="66173"/>
        <part id="66184"/>
        <part-sa-connection center_x="40" center_y="380" comp_id="66193" id="66185" main-connection-id="66209" name="FromPart_v2" size_x="16" size_y="16"/>
        <part-sa-connection center_x="40" center_y="140" comp_id="66171" id="66175" main-connection-id="66167" name="FromPart_s1" size_x="16" size_y="16"/>
        <part-sa-connection center_x="40" center_y="420" comp_id="66173" id="66196" main-connection-id="66166" name="FromPart_p2t" size_x="16" size_y="16"/>
        <part-sa-connection center_x="40" center_y="20" comp_id="66186" id="66180" main-connection-id="66207" name="FromPart_p1t" size_x="16" size_y="16"/>
        <part-sa-connection center_x="40" center_y="300" comp_id="66189" id="66170" main-connection-id="66211" name="FromPart_p2" size_x="16" size_y="16"/>
        <part-sa-connection center_x="40" center_y="60" comp_id="66174" id="66182" main-connection-id="66162" name="FromPart_v1" size_x="16" size_y="16"/>
        <part-sa-connection center_x="40" center_y="340" comp_id="66184" id="66203" main-connection-id="66208" name="FromPart_h2a" size_x="16" size_y="16"/>
        <part-sa-connection center_x="320" center_y="180" comp_id="66177" id="66235" main-connection-id="65894" name="ToPart_13" size_x="16" size_y="16"/>
        <part-sa-connection center_x="40" center_y="100" comp_id="66199" id="66183" main-connection-id="66165" name="FromPart_h1a" size_x="16" size_y="16"/>
    </subassembly>
</subassembly-extension>
